# jj40

![jj40](https://ae01.alicdn.com/kf/HTB18bq6bOERMeJjSspiq6zZLFXar.jpg?size=359506&height=562&width=750&hash=663a22d0109e2416ec8f54a7658686da)

A compact 40% (12x4) ortholinear keyboard kit made and KPRepublic on AliExpress.

* Keyboard Maintainer: [QMK Community](https://github.com/qmk)
* Hardware Supported: Atmega32A
* Hardware Availability: [AliExpress](https://www.aliexpress.com/store/product/jj40-Custom-Mechanical-Keyboard-40-PCB-programmed-40-planck-layouts-bface-firmware-gh40/3034003_32828781103.html)

Make example for this keyboard (after setting up your build environment):

    make jj40:default

Flashing example for this keyboard ([after setting up the bootloadHID flashing environment](https://docs.qmk.fm/#/flashing_bootloadhid))

    make jj40:default:flash

**Reset Key**: Hold down the *Top Right Key* key, commonly programmed as *Backspace* while plugging in the keyboard.

See the [build environment setup](https://docs.qmk.fm/#/getting_started_build_tools) and the [make instructions](https://docs.qmk.fm/#/getting_started_make_guide) for more information. Brand new to QMK? Start with our [Complete Newbs Guide](https://docs.qmk.fm/#/newbs).
