# Kabe Don 980

![Kabe Don 980](http://qungz.photo.store.qq.com/qun-qungz/V53LJWsQ407RKV3X7gmf3M0Ih23R00WB/V5bCQA1OTY5NTEwNjOx0B5fOCOlAQ!!/800?w5=2133&h5=1599&rf=viewer_421)

A mechanical keyboard PCB in the same layout as the Leopold FC980M, sold by Kabe Don Peripherals on Taobao.
This PCB  use Kailh hot swap sockets.
KabeDon980  Includes RGB   Underglow.
Aluminium Alloy and Translucent Case.

* Keyboard Maintainer:  [370490639](https://github.com/370490639)
* Hardware Supported: Kabe Don 980
* Hardware Availability: [Kabe Don 980](https://item.taobao.com/item.htm?spm=a1z10.1-c.w4023-17458066155.8.81406bd0J97pHX&id=614156027788)

Make example for this keyboard (after setting up your build environment):

    make kabedon/kabedon980:default

See the [build environment setup](https://docs.qmk.fm/#/getting_started_build_tools) and the [make instructions](https://docs.qmk.fm/#/getting_started_make_guide) for more information. Brand new to QMK? Start with our [Complete Newbs Guide](https://docs.qmk.fm/#/newbs).
