# bm40hsrgb

![BM40 RGB](https://rgoulter.com/images/keyboards/bm40rgb/bm40rgb_large.jpg)

An ortholinear 40% hotswap keyboard with per-key RGB in-switch LEDs and RGB Backlighting, from KP Republic.

This firmware was originally taken from a kbfirmware.json and manually converted. You may find the original `.json` files [here](https://drive.google.com/drive/folders/1tlTHQIFcluK2mjZ4UbbKCsdRLgSRSPw6).

* Keyboard Maintainer: [rgoulter](https://github.com/rgoulter)
* Hardware Supported: bm40hsrgb PCB
* Hardware Availability: [KPRepublic](https://www.aliexpress.com/item/4001147779116.html)

Make example for this keyboard (after setting up your build environment):

    make bm40hsrgb:default

Flashing example for this keyboard:

    make bm40hsrgb:default:flash

See the [build environment setup](https://docs.qmk.fm/#/getting_started_build_tools) and the [make instructions](https://docs.qmk.fm/#/getting_started_make_guide) for more information. Brand new to QMK? Start with our [Complete Newbs Guide](https://docs.qmk.fm/#/newbs).
