# Adi's DZ65RGB Layout
![Layout Visual](https://i.imgur.com/xuFkvVI.png)

This layout modifies the extra row on the right and makes some of the key bindings easier to reach on Layer 1.
## Step by Step
1. Build your Firmware: run build command in directory
```make dztech/dz65rgb/v1:adi```
2. Flash your Firmware:
    * Open QMK Toolbox Application
    * Open firmware file: dztech_dz65rgb_v1_adi.bin
    * Unplug keyboard USB-C, and hold the ESC key while plugging it back in
    * Check that QMK Toolbox displays: *** STM32 device connected. 
    * Hit the flash button!
