# kanu

![kanu](https://i.imgur.com/8JoH7wAl.jpg)

Kanu PCB, compatible Canoe keyboard V1.

* Keyboard Maintainer: [Team Mechlovin'](https://github.com/mechlovin)
* Hardware Supported: Canoe V1
* Hardware Availability: [Geekhack GB](https://geekhack.org/index.php?topic=106810.0), [Reddit GB](https://www.reddit.com/r/mechmarket/comments/gxtgio/gb_mechlovin_kanu_canoe_v1_compatible_pcb_plates/)


Make example for this keyboard (after setting up your build environment):

    make mechlovin/kanu:default

See the [build environment setup](https://docs.qmk.fm/#/getting_started_build_tools) and the [make instructions](https://docs.qmk.fm/#/getting_started_make_guide) for more information. Brand new to QMK? Start with our [Complete Newbs Guide](https://docs.qmk.fm/#/newbs).

**Reset Key:** To put the Kanu into bootloader, hold esc key while plugging in. 
