# Aplx2

![Front](https://i.imgur.com/cN4WfaQl.jpg)  
   
A simple 2% keyboard for osu!. Designed to be assembled as a sandwich with a Pro Micro, using M3 x 16mm screws, your choice of MX- or Alps-compatible switches, and 1N4148 diodes.   

**Layout:**  
The default layout is: Z , X .
Used pins can be found in `config.h`. All ProMicro pins can be found [here](https://cdn.sparkfun.com/datasheets/Dev/Arduino/Boards/ProMicro16MHzv1.pdf).

* Keyboard Maintainer: [Aplyard](https://github.com/Aplyard)
* Hardware Supported: Pro Micro (ATmega32U4)
* Hardware Availability: [GitHub](https://github.com/Aplyard/Aplx2), [Thingiverse](https://www.thingiverse.com/thing:4294608)

Make example for this keyboard (after setting up your build environment):

     make handwired/aplx2:default

See the [build environment setup](https://docs.qmk.fm/#/getting_started_build_tools) and the [make instructions](https://docs.qmk.fm/#/getting_started_make_guide) for more information. Brand new to QMK? Start with our [Complete Newbs Guide](https://docs.qmk.fm/#/newbs).

---  
**Designed in:**  
Fusion360     
[Keyboard Plate & Case Builder](http://builder.swillkb.com/)  
 

**Usefull Links:**  
[Qmk Online Configurator](https://config.qmk.fm/#)  

**Alternatives of qmk that worked for me:**  
[Keyboard Layout Editor](http://www.keyboard-layout-editor.com/#/)   
[Firmware Builder](https://kbfirmware.com/)      

---   
