# The PCB testing keymap for Polaris

LED control keys are placed on the numrow.  
Mainly for factory testing use only.  
  
ESC = Backlight Toggle  
1   = Backlight Step  
  
5    = RGB Toggle  
6    = RGB Mode Cycle  
7    = RGB Hue Increase  
8    = RGB Hue Decrease  
9    = RGB Saturation Increase  
0    = RGB Saturation Decrease  
MINS = RGB Value Increase  
EQL  = RGB Value Decrease  
