# [n]87

![n87](https://i.imgur.com/EAIGP1r.jpg)

A TKL pcb that supports standard, tsangan and symmetrical standard bottom row

* Keyboard Maintainer: [Neil Brian Ramirez](https://github.com/NightlyBoards)
* Hardware Supported: atmega32u4

Make example for this keyboard (after setting up your build environment):

    make nightly_boards/n87:default

See the [build environment setup](https://docs.qmk.fm/#/getting_started_build_tools) and the [make instructions](https://docs.qmk.fm/#/getting_started_make_guide) for more information. Brand new to QMK? Start with our [Complete Newbs Guide](https://docs.qmk.fm/#/newbs).
