# DudeOfAwesome's Preonic layout

![Preonic Layout](https://i.imgur.com/EC42Pnw.png)

## Features

- Base Layers
    - QWERTY
    - Workman
    - Dvorak
    - Colemak
- Numpad layer
    ![numpad layer](https://i.imgur.com/IH8sWmQ.png)
- Audio

## Building and flashing

1. Put your board in DFU mode with either the button on the bottom, or with a software key in your current firmware
1. Flash:
    ```bash
    $ make preonic/rev2:dudeofawesome:dfu
    ```
