# reviung34

![REVIUNG34 SPLIT](https://github.com/gtips/reviung/blob/master/reviung34split/image/REVIUNG34.jpg)  

The REVIUNG34 SPLIT is 34-key split ortholinear keyboard.  
Use one ProMicro.  
And connect the left and right keyboards using a LAN cable.  

Keyboard Maintainer: [gtips](https://github.com/gtips)  
Hardware Supported: The REVIUNG34 PCBs, Pro Micro supported  
Hardware Availability: [PCB & Case Data](https://github.com/gtips/reviung/tree/master/reviung34split)  

Make example for this keyboard (after setting up your build environment):

    make reviung34:default

See the [build environment setup](https://docs.qmk.fm/#/getting_started_build_tools) and the [make instructions](https://docs.qmk.fm/#/getting_started_make_guide) for more information. Brand new to QMK? Start with our [Complete Newbs Guide](https://docs.qmk.fm/#/newbs).

