# TR60W

![TR60W](https://i.imgur.com/Ez2T2Te.jpg)

This is the hotswap PCB supplied by Triangle Labs with their TR60 case, featuring four RGB LEDs around the Escape key, USB-C, and SMD single-color backlighting.

* Keyboard Maintainer: [Joule-Flow](https://github.com/Joule-Flow)
* Hardware Supported: TR60W PCB, ATmega32U4
* Hardware Availability: Group-buy by [Triangle Labs](https://geekhack.org/index.php?topic=96378.0)

Make example for this keyboard (after setting up your build environment):

    make tr60w:default

Or use my personal settings:

    make tr60w:joule-flow

See the [build environment setup](https://docs.qmk.fm/#/getting_started_build_tools) and the [make instructions](https://docs.qmk.fm/#/getting_started_make_guide) for more information. Brand new to QMK? Start with our [Complete Newbs Guide](https://docs.qmk.fm/#/newbs).
