# Stream Cheap

An ortholinear macropad, available in 2x3, 2x4, and 2x5 sizes.

Hardware:
  * 3d printed switch plate
  * 6-10 key switches
  * 3d printed case
  * Handwired in Direct Pins mode (i.e. all switches share a common GND and are wired to their own pin)
  * Uses a Pro Micro
  * Includes a reset switch accessible by a hole on the bottom

* Keyboard Maintainer: [hartk1213](https://github.com/hartk1213)
* Hardware Supported: Pro Micro
* Hardware Availability: [Thingiverse](https://www.thingiverse.com/thing:4497991)

Make example for this keyboard (after setting up your build environment):

    make handwired/stream_cheap/2x3:default
    make handwired/stream_cheap/2x4:default
    make handwired/stream_cheap/2x5:default

See the [build environment setup](https://docs.qmk.fm/#/getting_started_build_tools) and the [make instructions](https://docs.qmk.fm/#/getting_started_make_guide) for more information. Brand new to QMK? Start with our [Complete Newbs Guide](https://docs.qmk.fm/#/newbs).
