# ergoslab

![ergoslab](https://raw.githubusercontent.com/tomsaleeba/ergoslab/master/ergoslab.jpg)


A split ergo 5x6 keyboard with hotswap sockets and a heap of thumb keys designed
by Tom Saleeba. [More info on the GitHub
Repo](https://github.com/tomsaleeba/ergoslab).

**Status** The ergoslab is currently being beta-tested.

* Keyboard Maintainer: [Tom Saleeba](https://github.com/tomsaleeba)
* Hardware Supported: Pro Micro (ATmega32U4)
* Hardware Availability: gerbers are available from the [releases page on the
GitHub repo](https://github.com/tomsaleeba/ergoslab/releases). Get them
manufactured at your favourite PCB house. I used JLCPCB.


Make example for this keyboard (after setting up your build environment):

    make ergoslab:default

Example of flashing this keyboard:

    make ergoslab:default:flash

See the [build environment setup](https://docs.qmk.fm/#/getting_started_build_tools)
and the [make instructions](https://docs.qmk.fm/#/getting_started_make_guide)
for more information. Brand new to QMK? Start with our
[Complete Newbs Guide](https://docs.qmk.fm/#/newbs).

A build guide for this keyboard can be found here: [Build
Guide](https://github.com/tomsaleeba/ergoslab/blob/master/build-guide.md)
