# 素 - Shiro 

![Shiro](https://cdn.discordapp.com/attachments/536423734144401422/597447002288291861/P7070070_cp.jpg)

これは日本の名刺(55mmx91mm)に、3x5の15キーを詰め込んだとても小さいキーパッドです。

This product is a 3x5 very small keypad.
It is made in 55mm x 91mm according to the Japanese business card.

Keyboard Maintainer: [T.Shinohara](https://github.com/ShinoharaTa)  
Hardware Supported:  The Shiro PCBs, ProMicro supported. Using only Kailh Low Profile Switches.  
Hardware Availability: [Booth (Japanese Site)](https://shino3.booth.pm/items/1444895)  
日本国内ではBoothで入手できます: [Booth (Japanese Site)](https://shino3.booth.pm/items/1444895)

![Shiro-backside](https://cdn.discordapp.com/attachments/536423734144401422/597464086640328724/20190707_033520.jpg)

Make for this keyboard default keymap (after setting up your build environment):

    make shiro:default

Make for this keyboard build check keymap (after setting up your build environment):

    make shiro:check

See the [build environment setup](https://docs.qmk.fm/#/getting_started_build_tools) and the [make instructions](https://docs.qmk.fm/#/getting_started_make_guide) for more information. Brand new to QMK? Start with our [Complete Newbs Guide](https://docs.qmk.fm/#/newbs).

[Build guide - Japanese](https://github.com/ShinoharaTa/keyboards/blob/master/Shiro/manual/build_guide_ja.md)  