# flatbread60

![flatbread60](https://i.imgur.com/kIPP0JKl.jpg)

This is a custom PCB made by a hobbiest, and it has an ortholinear 60 key layout. Flatbread60 supports Pro Micro and its wireless variants, such as Blue Micro. A battery switch slot and extra pinout is on the board.  

* Keyboard Maintainer: [noclew](https://github.com/noclew)
* Hardware Supported: flatbread60 PCB
* Hardware Availability: Not commercially available, but the board fabricaion file will be uploaded in the near future.

Make example for this keyboard (after setting up your build environment):

    make nckiibs/flatbread60:default

Flashing example for this keyboard:
    
    make nckiibs/flatbread60:default:flash

See the [build environment setup](https://docs.qmk.fm/#/getting_started_build_tools) and the [make instructions](https://docs.qmk.fm/#/getting_started_make_guide) for more information. Brand new to QMK? Start with our [Complete Newbs Guide](https://docs.qmk.fm/#/newbs).
