# runner3680

![runner3680](https://github.com/omkbd/Runner3680/blob/master/Picture/Runner3680.jpg)

A split ortholinear keyboard. Each half is a 5x8 arrangement, with breakable pieces to allow the number of rows to be customized between 3 to 5, and the number of columns to be between 6 to 8.  

Keyboard Maintainer: [omkbd](https://github.com/omkbd) [@omkbd](https://twitter.com/omkbd)  
Hardware Supported: Runner3680, Pro Micro ATmega32u4    
Hardware Availability: Order your own [yourself](https://github.com/omkbd/Runner3680)

Make example for this keyboard (after setting up your build environment):

    make runner3680/5x8:default

See the [build environment setup](https://docs.qmk.fm/#/getting_started_build_tools) and the [make instructions](https://docs.qmk.fm/#/getting_started_make_guide) for more information. Brand new to QMK? Start with our [Complete Newbs Guide](https://docs.qmk.fm/#/newbs).
