# h60

![h60](https://live.staticflickr.com/65535/49952697531_2efeaa0bd6_k.jpg)

A GH60 form factor PCB for 60% keyboards. Uses a USB Type C connector.

* Keyboard Maintainer: [hineybush](https://github.com/hineybush)
* Hardware Supported: h60
* Hardware Availability: [hiney.cc](https://hiney.cc)

Make example for this keyboard (after setting up your build environment):

    make hineybush/h60:default

See the [build environment setup](https://docs.qmk.fm/#/getting_started_build_tools) and the [make instructions](https://docs.qmk.fm/#/getting_started_make_guide) for more information. Brand new to QMK? Start with our [Complete Newbs Guide](https://docs.qmk.fm/#/newbs).
