# O4L 5x12

A ortholinear 5x12 keyboard made and sold by Keycapsss. [More info at Keycapsss.com](https://keycapsss.com).

<img src="https://i.imgur.com/5p8rDme.jpg" height="500px">

## Features:

- MX and Choc switch support
- RGB Underglow (12x SK6812MINI)
- USB-C
- PCB shape, reset button and mounting holes position same as Preonic Rev3
- Pro Micro as controller

---

- Keyboard Maintainer: BenRoe [GitHub](https://github.com/BenRoe) / [Twitter](https://twitter.com/ben_roe)  
- Hardware Supported: Pro Micro  
- Hardware Availability: [Keycapsss.com](https://keycapsss.com)  



Make firmware .hex for this keyboard (after setting up your build environment):

    make keycapsss/o4l_5x12:default

Example of flashing this keyboard (or use [QMK Toolbox](https://github.com/qmk/qmk_toolbox)):

    make keycapsss/o4l_5x12:default:avrdude

See the [build environment setup](https://docs.qmk.fm/#/getting_started_build_tools) and the [make instructions](https://docs.qmk.fm/#/getting_started_make_guide) for more information. Brand new to QMK? Start with our [Complete Newbs Guide](https://docs.qmk.fm/#/newbs).
