# squiggle

![squiggle](https://i.imgur.com/5UhvDsjl.jpg)

It's a keyboard family which has the following requirements:

-  5 columns per hand.
-  At most 3 keys for each side's thumb row.
-  No numrow.
-  Split.
-  Symmetric.

* Keyboard Maintainer: [ibnuda](https://github.com/ibnuda)
* Hardware Supported: Atmega32u4.
* Hardware Availability: [shop](https://dactyl.bigcartel.com/product/squiggle-keyboard-kit) or [repo](https://github.com/ibnuda/squiggle).

Make example for this keyboard (after setting up your build environment):

    make squiggle:default

See the [build environment setup](https://docs.qmk.fm/#/getting_started_build_tools) and the [make instructions](https://docs.qmk.fm/#/getting_started_make_guide) for more information. Brand new to QMK? Start with our [Complete Newbs Guide](https://docs.qmk.fm/#/newbs).
