# HolySwitch Co Southpaw75

60% Keyboard with numpad on the left side. 

This is the USB C, with pre soldered components and was a US exclusive sold through HolySwitch Co. The international 
version was sold with a pro micro. 

Firmware on the international version is not compatible with this PCB, and firmware for this PCB is not compatible 
with the international version. 

* Keyboard Maintainer: [Drewpyun](https://github.com/drewpyun), [MechMerlin](https://github.com/mechmerlin)
* Hardware Supported: Southpaw75
* Hardware Availability: [HolySwitch Co.](https://holyswitch.co/collections/group-buys/products/southpaw75)

Make example for this keyboard (after setting up your build environment):

    make holyswitch/southpaw75:default

Flashing example for this keyboard:

    make holyswitch/southpaw75:default:flash

See the [build environment setup](https://docs.qmk.fm/#/getting_started_build_tools) and the [make instructions](https://docs.qmk.fm/#/getting_started_make_guide) for more information. Brand new to QMK? Start with our [Complete Newbs Guide](https://docs.qmk.fm/#/newbs).
