# RGB backlight for MinOrca

![wiring](https://i.imgur.com/jyYyiSS.jpg)

Example of adding WS2812b LEDs to a MinOrca.

http://www.40percent.club/2016/08/tiny-whale.html

The keymap is a work in progress. The RGB functions are accessed by holding down the TAB key. 

Shortcut | Function
:------- | :-----
Tab + Z  | Toggle on/off
Tab + X  | Mode
Tab + C  | Hue+
Tab + V  | Hue-
Tab + B  | Saturation+
Tab + N  | Saturation-
Tab + M  | Brightness+
Tab + ,  | Brightness-

## Example wiring:

WS2812 data pin is connected to D5

![wiring](https://i.imgur.com/CFBf71F.jpg)
![wiring closeup](https://i.imgur.com/VJogRoj.jpg)
